Model: UNIDEN SDS200

Downgrade to 1.23.15  

The SUB also need to be downgrade at the same time.
If you downgrade to this version, you must also downgrade Sub to V1.03.06 at the same time.


Caution: Do not put different firmware versions on the SD card at the same time. If there are different versions, the upload will not start or will not be uploaded correctly, so please be sure to upload only one version. 　

If you accidentally delete two dat files already included in the SD card that are not related to Firmware, SDS200 will not start properly. If you accidentally delete these files, you can restore them by executing "Clear User Data..." via Sentinel, but all User Data will be lost.

Please back up contents in SD card and your settings via Sentinel just in case.

Steps:
Turn On the SDS200
Connect the Windows PC and SDS200 with a USB cable. 

SDS200 Screen:
++++++++++++++++++++
USB Cable Detected
Select USB mode

Mass Strage = "E"
Serial Port ="."
++++++++++++++++++++

Press "E(Yes)" key to select "Mass Storage" 

SDS200 Screen:
++++++++++++++++++++
USB Mass Storage
++++++++++++++++++++

Open Windows Explorer. 
A folder for Removable disk "BCDx36HP" will appear.
Open the "firmware" folder inside "BCDx36HP" folder.

here are two "dat" files inside.　Do not touch these files.

++++++++++++++++++++

Copy and paste "SDS200_V1_23_15.bin"and "SDS200-SUB_V1_03_06.firm" to this folder. 

Windows Explorer Screen:
+++++++++++++++++++++

Removable disk (X:)  X = varies depending of PC settings. 
BCDx36HP
 L activity_log
   .
   .
   firmware <--- Open this folder.
    L CitiTable_V00_00.dat <-- Do not touch.  
      ZipTable_V00_00.dat <-- Do not touch.
      SDS200_V1_23_15.bin <-- Copy main firmware to here*.
      SDS200-SUB_V_03_06.firm <-- Copy sub firmware to here**.	

++++++++++++++++++++++

* Do not upload multiple main firmware. 
** Do not upload multiple sub firmware. 

After the copy is complete, reset the power, update will start automatically. 
!!! Do not turn off the power until the upload is complete !!!

Note: After the process is finished, these firmware files will be automatically deleted from the "fimware" folder.


Caution: Please use these files on your risk. Uniden is not responsible for any damage caused by these processes.